Dual port faceplate 45x45

Dual port faceplate 45x45

accepts modules type AMJ-K, AMJ-S, UMJ-K;

to be used in 45x45mm switch and socket outlet systems;

sloped patch cord exit;

spring-loaded shutters;

4 latches for secure fastening;

labelling field with transparent cover;

icons to depict applications above the labelling field included;

Features:

Material: ABS

Colour: white

Dimensions: 45x45mm (WxH)

Protrusion: ≤ 25.75mm

Manufacturer: Telegärtner

Type: Faceplate 45x45 French style

Part No.: 100021428