**Fiber optic distributor IP68 for pre-terminated fiber optic cables**

Durable plastic housing IP68 rated

for indoor and outdoor use,

mounting opitions: on walls, on ceilings, in floors, on poles and direct burial

round housing ensures bending radii of cables and fibers

sealing in circumferential groove in cover;

Model for pre-terminated fiber optic cables with

ODS/M20 cable spliters

with 2 adapters for ODS/M20 cable splitters

Features:

Housing:

- Dimensions: max. 220x185mm (LxW)

- Heigth: max. 65mm

- Rating: min. IP68, indoor and outdoor use

- Material: PPE, UV-resistant, flame retardant

- Colour: black

- Cable entries: 4 ea. for cables with an outer diameter

 of 4 to 13 mm;

 2 entries open

 2 entries closed, can be opended on-site

- Temperature range: -40 to +85 °C

- Locking: bolted, lead-sealable

Distributor comes with

- 6x adaptors SC Duplex

- 6x adaptors LC Duplex

- 12x adaptors LC Duplex

[delete as applicable!]

Adaptors with ceramic sleeve,

housing colour

- blue

- green

- beige

- black

- aqua

- violet

- lime green

[delete as applicable!]

Distributor comes with:

- 2 adapters for ODS/M20 cable splitters

Manufacturer: Telegärtner

Type: TOC ODB 68

Part No.: H02050A0311\_plus\_adaptors