Installation cable S/FTP 2x(4x2xAWG23/1), C.7, D-111

Installation cable S/FTP 2x(4x2xAWG23/1), for EN 50173 and ISO/IEC 11802 class F links or higher;

RL ≥ 21dB@1GHz,

to ensure high wire eccentricity;

meets the specifications of EN 50288-4-1;

cable jacket made of halogen-free, flame retardant material;

reaction to fire class Dca-s2,d1,a1 or better according to European CPR;

fire retardant according to ISO/IEC 60332-1;

segregation classification “d” of EN 50174-2:2018-10;

Fire load: ≤ 0.28 kWh/m;

Cable outer diameter: ≤ 7.0 x 15.6 mm;

Colour of cable jacket: blue;

Manufacturer: Telegärtner

Type: AMJ 1000

Part No.: L02002A0182