**19” 24 port module carrier 1 HU, grey**

Module carrier made of metal for 19” rack mount;

panel accepts a minimum of 24 RJ45 couplers and modules;

ports labeled 1 to 24 on panel;

comes with 24 RJ45 couplers Cat.6A with jacks on the front and the rear, for applications according to ISO/IEC 11801-1, Annex E (10 Gbit/s, PoE Type 2);

optimized contact design to avoid sparcs in the area of data transmission;

coupler housing has a flat-pin contact for individual bonding;

The channel consisting of this coupler and the connectorized cable as specified elsewhere in this tender has to meet or exceed the specifications of ISO/IEC 11801-1 channel class EA;

**Features:**

RJ45 coupler

 Depth: ≤ 38.2 mm

 Width: ≤ 17.0 mm

 Performance: for ISO/IEC 11801-1 class EA

 Plug compatibility: RJ45, RJ12 and RJ11 plugs,

 protection against over-

 bending the contacts

 Mating cycles: ≥ 750

 Cable diameter: ≤ 9 mm

 Contacts: 8

...Wiring scheme: 1:1

 Contact design: Optimized design, evidence

 provided by data sheet

 Bonding connection: 6.3 mm DIN 46342-1

Module carrier:

 Depth: ≤ 28 mm

 Material: sheet steel, powder coated

 Color: light grey like RAL 7035

 Number of ports: ≥ 24

 Number of cable ties: ≥ 24

Manufacturer: Telegärtner

Type: 19“ module carrier 1U

Part No.: 100007007