19” 24 port module carrier 1HU, angled ports, black

Module carrier made of metal for 19” rack mount, with integrated cable management;

pre-installed bonding wire;

ports labeled 1 to 24 on panel;

latch of plug pointing upwards when connected on all ports;

two rows of staggered ports,

ports have 15° angle, ports 1 to 12 pointing to the left, ports 13 to 24 pointing to the right.

Features:

Depth: ≤ 150mm

Material of module carrier:

- Front: sheet steel, powder coated

- Back: sheet steel, galvanized

- Monting plate: sheet steel, powder coated

Temperature range: -40°C to +70°C

Manufacturer: Telegärtner

Type: Modulträger AMJ/UMJ

Part No.: 100021505