RJ45 coupler Cat.6A

RJ45 coupler Cat.6A, for applications according to ISO/IEC 11801-1, Annex E (10 Gbit/s, PoE Type 2);

optimized contact design to avoid sparcs in the area of data transmission;

Features:

Depth: ≤ 38.2 mm

Width: ≤ 17.0 mm

Performance: for ISO/IEC 11801-1 class EA PL

Plug compatibility: RJ45, RJ12 and RJ11 plugs,

 protection against overbending

 the contacts

Mating cycles: ≥ 750

Contacts: 8

Wiring scheme: 1.1

Contact design: Optimized design, evidence

 provided by data sheet

Bonding connection: 6.3 mm DIN 46342-1

Manufacturer: Telegärtner

Type: AMJ Coupler K Cat.6A

Part No.: 100023165