Installation cable U/UTP 4x2xAWG23/1, Cat.6A, D-221

Installation cable U/UTP 4x2xAWG23/1, for EN 50173 or ISO/IEC 11801 class EA links or higher;

meets the specifications of EN 50288-11-1;

non-metallic cross-filler element for reliable separation of wire pairs;

cable jacket made of halogen-free, flame retardant material;

reaction to fire class Dca-s2,d2,a1 or better according to European CPR;

fire retardant according to ISO/IEC 60332-1-2;

Fire load: ≤ 784 MJ/km

Cable outer diameter: ≤ 7.2 mm

Cable jacket colour: blue

Manufacturer: Telegärtner

Type: UMJ 500

Part No.: 100124686