**6-Port Mini Distributor Cat6A, HS**

Metallic housing for din rail;

Cable management for a minimum of six cables;

integrated PCB with 6 jacks Cat6A;

pre-installed bonding wire;

RJ45 jacks Cat.6A, which meet or exceed the specifications of IEC 60603-7-51;

on one PCB with IDC terminals;

for applications according to ISO/IEC 11801-1, Annex E (10 Gbit/s, PoE Type 4);

eligible for 4PPoE (PoE Types 3 and 4), tested on the basis of IEC 60512-99-002 and EN 60512-9-3;

IDC contacts eligible for solid and stranded wires;

strain relief with cable ties;

comes with minimum two mounting rail adaptors

Features:

Jacks: Cat6A gem. EN 60603-7-51

- Compatibility: RJ45-/12-/11-plugs, protection against overbending the contacts

- Mating cycles: ≥ 750

- Contacts: 8

- Wire connection: IDC

- Wire diameter: 0.7-1.6mm

- Reusable IDC: ≥ 50

- Dimension: solid: AWG26/1–22/1

- Pin/pair assignments: T568A and B

Housing:

- Dimensions: ≤ 95.8x111.6x22.6mm (HxBxT)

- Material: sheet steel, varnished

- Jack housing: sheet steel, zinc plated

- Din rail clamp: DIN 35mm rail

Manufacturer: Telegärtner

Type: MPD 6-HS K Cat6A

Part No.: J02021A0055