RJ45 patch cord Cat.6A

Patch cord for all class EA applications of EN 50173-1, annex F and ISO/IEC 11801-2, annex E, including 10 Gigabit Ethernet and PoE+; UL listed;

PVP quality assurance certified;

made of S/FTP 4x2xAWG27/7 Cat.7 (600MHz) cable and

MP8 type plug;

plug has moulded boot and latch protection, colour matching cable jacket colour;

boot has groves to fix mounting clip of RFID transponder for AIM functionality;

cord has to be available with 90°, 180° or 270° cable boot;

cord length printed on cable boot;

wires have to be made of high-quality copper only, proof by data sheet; copper-clad aluminum wires are NOT accepted.

Features:

Length:

Colour:

Pinout:

Boot:

Plug:

-Performance: IEC 60603-7-51 Cat.6A

Cable:

-Type: S/FTP 4x2xAWG27/7

-Wire material: Cu

-Performance: EN 50288-4-2 Cat.7

-Outer diameter: ≤ 5.8 mm

-Jacket materiel: LSZH

-Flame retardancy: EN60332-1, UL444CM

Appropriate mounting clip:

-Inner dimensions: (WxH):10.8 x 8.65 mm

Manufacturer: Telegärtner

Type: MP8 FS500 LSZH

Part No.: 100007964