19” 24 port module carrier flex 1 HU, white

Module carrier made of metal for 19” rack mount, with integrated cable management with 24 cable fixation points;

pre-installed bonding wire;

bonding wire connection by cable eye for M6 screw;

front panel with 24 snap-in bezels with shutters and labeling field with clear label retainer;

accepts modules type AMJ-K;

Features:

Depth: ≤ 118 mm

Material of module carrier: sheet steel, ST1203,

 thickness ≥ 1.5 mm, powder coated

Colour: light grey like RAL 7035

Material of bezel: ABS

Colour of bezel: pure white

Bonding wire: conductor area ≥ 4 mm²

Bonding wire: length ≥ 300 mm

Bonding connection DIN 46234

Manufacturer: Telegärtner

Type: Module carrier AMJ/UMJ

Part No.: 100021502